MIPS R4000 Microprocessor User's Manual G-1

R4000 Pinouts

G

This Appendix shows the pinouts for the three microprocessor configurations: R4000PC, R4000SC, and R4000MC.

NOTE: This entire Appendix, Appendix G, is new for the second edition.

Appendix G

G-2 MIPS R4000 Microprocessor User's Manual

G.1 Pinout of R4000PC

Figure G-1 shows the physical pinout of the R4000PC. Table G-1 lists the signal-to-pin correspondence.

Figure G-1 R4000PC Physical Pinout

• • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • •

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18

1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16 17 18

V U T R P N M L K J H G F E D C B A

V U T R P N M L K J H G F E D C B A

R4000 PC Pinout x Bottom

MIPS R4000 Microprocessor User's Manual G-3

Table G-1 Signal-to-Pin Correspondences for the R4000PC

†. This node has capacitors for the PLL premounted to the package.

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin ColdReset* T14 ExtRqst* U2 Fault* B16 NC U10 Vcc T9 IOIn T13 IOOut U12 Int*0 N2 Int*1 L3 Int*2 K3 Int*3 J3 Int*4 H3 Int*5 F2 JTCK H17 JTDI G16 JTDO F16 JTMS E16 MasterClock J17 MasterOut P17 ModeClock B4 ModeIn U4 NMI* U7 PLLCap0 ****^† PLLCap1 ****^† RClock0 T17 RClock1 R16 RdRdy* T5 Release* V5 Reset* U16 SyncIn J16 SyncOut P16 SysAD0 J2 SysAD1 G2 SysAD2 E1 SysAD3 E3 SysAD4 C2 SysAD5 C4 SysAD6 B5 SysAD7 B6 SysAD8 B9 SysAD9 B11 SysAD10 C12 SysAD11 B14 SysAD12 B15 SysAD13 C16 SysAD14 D17 SysAD15 E18 SysAD16 K2 SysAD17 M2 SysAD18 P1 SysAD19 P3 SysAD20 T2 SysAD21 T4 SysAD22 U5 SysAD23 U6 SysAD24 U9 SysAD25 U11 SysAD26 T12 SysAD27 U14 SysAD28 U15 SysAD29 T16 SysAD30 R17 SysAD31 M16 SysAD32 H2 SysAD33 G3 SysAD34 F3 SysAD35 D2 SysAD36 C3 SysAD37 B3 SysAD38 C6 SysAD39 C7 SysAD40 C10 SysAD41 C11 SysAD42 B13 SysAD43 A15 SysAD44 C15 SysAD45 B17 SysAD46 E17 SysAD47 F17 SysAD48 L2 SysAD49 M3 SysAD50 N3 SysAD51 R2 SysAD52 T3 SysAD53 U3 SysAD54 T6 SysAD55 T7 SysAD56 T10 SysAD57 T11 SysAD58 U13 SysAD59 V15 SysAD60 T15 SysAD61 U17 SysAD62 N16 SysAD63 N17 SysADC0 C8

G-4 MIPS R4000 Microprocessor User's Manual

Table G-1 (cont.) Signal-to-Pin Correspondences for the R4000PC

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin SysADC1 G17 SysADC2 T8 SysADC3 L16 SysADC4 B8 SysADC5 H16 SysADC6 U8 SysADC7 L17 SysCmd0 E2 SysCmd1 D3 SysCmd2 B2 SysCmd3 A5 SysCmd4 B7 SysCmd5 C9 SysCmd6 B10 SysCmd7 B12 SysCmd8 C13 SysCmdP C14 TClock0 C17 TClock1 D16 VCCOk M17 ValidIn* P2 ValidOut* R3 WrRdy* C5 VccP K17 VssP K16 Vcc A2 Vcc A4 Vcc A7 Vcc A9 Vcc A11 Vcc A13 Vcc A16 Vcc B18 Vcc C1 Vcc D18 Vcc F1 Vcc G18 Vcc H1 Vcc J18 Vcc K1 Vcc L18 Vcc M1 Vcc N18 Vcc R1 Vcc T18 Vcc U1 Vcc V3 Vcc V6 Vcc V8 Vcc V10 Vcc V12 Vcc V14 Vcc V17 Vss A3 Vss A6 Vss A8 Vss A10 Vss A12 Vss A14 Vss A17 Vss A18 Vss B1 Vss C18 Vss D1 Vss F18 Vss G1 Vss H18 Vss J1 Vss K18 Vss L1 Vss M18 Vss N1 Vss P18 Vss R18 Vss T1 Vss U18 Vss V1 Vss V2 Vss V4 Vss V7 Vss V9 Vss V11 Vss V13 Vss V16 Vss V18

MIPS R4000 Microprocessor User's Manual G-5

R4000 Pinouts

G.2 Pinout of R4000MC/SC Package Pinout

Figure G-2 shows the physical pinout of the R4000MC and SC. Table G-2 lists the signal-to-pin correspondence.

Figure G-2 R4000MC/SC Physical Pinout

• • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • • •

39 38 37 36 35 34 33 32 31 30 29 28 27 26 25 24 23 22 21 20 19 18 17 16 15 14 13 12 11 10 9 8 7 6 5 4 3 2 1

39 38 37 36 35 34 33 32 31 30 29 28 27 26 25 24 23 22 21 20 19 18 17 16 15 14 13 12 11 10 9 8 7 6 5 4 3 2 1

AW AU AR AN AL AJ AG AE AC AA W U R N L J G E C A AV AT AP AM AK AH AF AD AB Y V T P M K H F D B

AW AU AR AN AL AJ AG AE AC AA W U R N L J G E C A AV AT AP AM AK AH AF AD AB Y V T P M K H F D B

R4000 MC/SC 447 Pinout (bottom)

G-6 MIPS R4000 Microprocessor User's Manual

Table G-2 Signal-to-Pin Correspondences for the R4000MC/SC

†. Used only in the MC part. Must be tied to Vcc for the SC part. ‡. This node has capacitors for the PLL premounted to the package.

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin ColdReset* AW37 ExtRqst* AV2 Fault* C39 NC AV24 Vcc AV20 IOIn AV32 IOOut AV28 Int*0 AL1 IvdAck*^† AA35 IvdErr*^† AA39 JTCK U39 JTDI N39 JTDO J39 JTMS G37 MasterClock AA37 MasterOut AJ39 ModeClock B8 ModeIn AV8 NMI* AV16 PLLCap0 ****^‡ PLLCap1 ****^‡ RClock0 AM34 RClock1 AL33 RdRdy* AW7 Release* AV12 Reset* AU39 SC64Addr Y2 SCAPar0 U5 SCAPar1 U1 SCAPar2 P4 SCAdd1 AL5 SCAdd2 AG1 SCAdd3 AE7 SCAdd4 AC1 SCAdd5 AC5 SCAdd6 AC3 SCAdd7 AA1 SCAdd8 AB4 SCAdd9 AA5 SCAddr10 AA7 SCAddr11 AA3 SCAddr12 W3 SCAddr13 Y6 SCAddr14 W5 SCAddr15 W7 SCAddr16 W1 SCAddr17 U3 SCAddr0W AN7 SCAddr0X AN5 SCAddr0Y AM6 SCAddr0Z AL7 SCDCS* M6 SCDChk0 G19 SCDChk1 T34 SCDChk2 AP20 SCDChk3 AD34 SCDChk4 C19 SCDChk5 R37 SCDChk6 AU19 SCDChk7 AE37 SCDChk8 C17 SCDChk9 N37 SCDChk10 AU17 SCDChk11 AG37 SCDChk12 E19 SCDChk13 R35 SCDChk14 AR19 SCDChk15 AE35 SCData0 R3 SCData1 R7 SCData2 L5 SCData3 F8 SCData4 C9 SCData5 F12 SCData6 G15 SCData7 E17 SCData8 G21 SCData9 C25 SCData10 G25 SCData11 E29 SCData12 G31 SCData13 C35 SCData14 K36 SCData15 N35 SCData16 AE3 SCData17 AG5 SCData18 AK4 SCData19 AN9 SCData20 AU9 SCData21 AN13 SCData22 AT14 SCData23 AR17 SCData24 AT22

MIPS R4000 Microprocessor User's Manual G-7

Table G-2 (cont.) Signal-to-Pin Correspondences for the R4000MC/SC

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin SCData25 AU25 SCData26 AN27 SCData27 AR29 SCData28 AN31 SCData29 AR35 SCData30 AK36 SCData31 AG35 SCData32 T6 SCData33 L3 SCData34 L7 SCData35 E7 SCData36 G11 SCData37 E13 SCData38 E15 SCData39 G17 SCData40 C23 SCData41 F24 SCData42 E27 SCData43 D30 SCData44 C33 SCData45 E35 SCData46 L35 SCData47 R33 SCData48 AF4 SCData49 AJ3 SCData50 AJ7 SCData51 AP8 SCData52 AT10 SCData53 AR13 SCData54 AR15 SCData55 AT18 SCData56 AU23 SCData57 AT26 SCData58 AR27 SCData59 AN29 SCData60 AP32 SCData61 AN35 SCData62 AJ35 SCData63 AE33 SCData64 V4 SCData65 R5 SCData66 N5 SCData67 E5 SCData68 G9 SCData69 E11 SCData70 G13 SCData71 D14 SCData72 C21 SCData73 D22 SCData74 E25 SCData75 G27 SCData76 C31 SCData77 F32 SCData78 J35 SCData79 M34 SCData80 AC7 SCData81 AE5 SCData82 AG7 SCData83 AR5 SCData84 AR9 SCData85 AR11 SCData86 AN15 SCData87 AP16 SCData88 AU21 SCData89 AN23 SCData90 AR25 SCData91 AP28 SCData92 AU31 SCData93 AR33 SCData94 AL35 SCData95 AH34 SCData96 U7 SCData97 N3 SCData98 N7 SCData99 C5 SCData100 E9 SCData101 C11 SCData102 C13 SCData103 F16 SCData104 E21 SCData105 G23 SCData106 C27 SCData107 F28 SCData108 E31 SCData109 G33 SCData110 J37 SCData111 N33 SCData112 AD6 SCData113 AG3 SCData114 AJ5 SCData115 AU5 SCData116 AN11 SCData117 AU11 SCData118 AU13 SCData119 AN17 SCData120 AR21

G-8 MIPS R4000 Microprocessor User's Manual

Table G-2 (cont.) Signal-to-Pin Correspondences for the R4000MC/SC

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin SCData121 AP24 SCData122 AU27 SCData123 AT30 SCData124 AU33 SCData125 AN33 SCData126 AL37 SCData127 AG33 SCOE* N1 SCTCS* J1 SCTChk0 AN21 SCTChk1 AN19 SCTChk2 AU15 SCTChk3 AP12 SCTChk4 AU7 SCTChk5 AR7 SCTChk6 AH6 SCTag0 K4 SCTag1 G7 SCTag2 C7 SCTag3 D10 SCTag4 C15 SCTag5 D18 SCTag6 F20 SCTag7 E23 SCTag8 D26 SCTag9 C29 SCTag10 G29 SCTag11 E33 SCTag12 G35 SCTag13 L33 SCTag14 L37 SCTag150 P36 SCTag16 AF36 SCTag17 AJ37 SCTag18 AJ33 SCTag19 AN37 SCTag20 AU35 SCTag21 AR31 SCTag22 AU29 SCTag23 AN25 SCTag24 AR23 SCWrW* J5 SCWrX* J7 SCWrY* H6 SCWrZ* G5 Status0 U33 Status1 U35 Status2 V36 Status3 W35 Status4 W37 Status5 AC37 Status6 AC35 Status7 AC33 SyncIn W39 SyncOut AN39 SysAD0 T2 SysAD1 M2 SysAD2 J3 SysAD3 G3 SysAD4 C1 SysAD5 A3 SysAD6 A9 SysAD7 A13 SysAD8 A21 SysAD9 A25 SysAD10 A29 SysAD11 A33 SysAD12 B38 SysAD13 E37 SysAD14 G39 SysAD15 L39 SysAD16 AD2 SysAD17 AH2 SysAD18 AL3 SysAD19 AN3 SysAD20 AU1 SysAD21 AW3 SysAD22 AW9 SysAD23 AW13 SysAD24 AW21 SysAD25 AW25 SysAD26 AW29 SysAD27 AW33 SysAD28 AV38 SysAD29 AR37 SysAD30 AM38 SysAD31 AH38 SysAD32 R1 SysAD33 L1 SysAD34 H2 SysAD35 E1 SysAD36 C3 SysAD37 A5 SysAD38 A11 SysAD39 A15 SysAD40 A23

MIPS R4000 Microprocessor User's Manual G-9

Table G-2 (cont.) Signal-to-Pin Correspondences for the R4000MC/SC

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin SysAD41 A27 SysAD42 A31 SysAD43 A35 SysAD44 C37 SysAD45 B39 SysAD46 H38 SysAD47 M38 SysAD48 AE1 SysAD49 AJ1 SysAD50 AM2 SysAD51 AR1 SysAD52 AU3 SysAD53 AW5 SysAD54 AW11 SysAD55 AW15 SysAD56 AW23 SysAD57 AW27 SysAD58 AW31 SysAD59 AW35 SysAD60 AU37 SysAD61 AR39 SysAD62 AL39 SysAD63 AG39 SysADC0 A17 SysADC1 R39 SysADC2 AW17 SysADC3 AD38 SysADC4 A19 SysADC5 T38 SysADC6 AW19 SysADC7 AC39 SysCmd0 G1 SysCmd1 E3 SysCmd2 B2 SysCmd3 B12 SysCmd4 B20 SysCmd5 B24 SysCmd6 B28 SysCmd7 B32 SysCmd8 A37 SysCmdP H34 TClock0 H34 TClock1 J33 VCCOk AE39 ValidIn* AN1 ValidOut* AR3 WrRdy* A7 VccSense W33 VssSense U37 VccP AA33 VssP Y34 Vcc A39 Vcc B6 Vcc B10 Vcc B18 Vcc B26 Vcc B34 Vcc D4 Vcc D8 Vcc D16 Vcc D24 Vcc D32 Vcc D36 Vcc F2 Vcc F14 Vcc F22 Vcc F30 Vcc F38 Vcc H4 Vcc H36 Vcc K6 Vcc K38 Vcc Y38 Vcc AB2 Vcc AB34 Vcc AD4 Vcc AD36 Vcc AF6 Vcc AF38 Vcc AK2 Vcc AK34 Vcc AM4 Vcc AM36 Vcc AP2 Vcc AP10 Vcc AP18 Vcc AP26 Vcc AP38 Vcc AT4 Vcc AT8 Vcc AT16 Vcc AT24 Vcc AT32 Vcc AT36 Vcc AV6 Vcc AV14

G-10 MIPS R4000 Microprocessor User's Manual

Table G-2 (cont.) Signal-to-Pin Correspondences for the R4000MC/SC

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin

R4000 PC Pkg Function Pin Vcc AV22 Vcc AV30 Vcc AV34 Vcc AW1 Vcc AW39 Vss B4 Vss B14 Vss B22 Vss B30 Vss B36 Vss D2 Vss D6 Vss D12 Vss D20 Vss D28 Vss D34 Vss D38 Vss F4 Vss F6 Vss F10 Vss F18 Vss F26 Vss F34 Vss F36 Vss K2 Vss K34 Vss M4 Vss M36 Vss P6 Vss P38 Vss V2 Vss Y4 Vss Y36 Vss AB6 Vss AB36 Vss AB38 Vss AF2 Vss AF34 Vss AH4 Vss AH36 Vss AK6 Vss AK38 Vss AP4 Vss AP6 Vss AP14 Vss AP22 Vss AP30 Vss AP34 Vss AP36 Vss AT2 Vss AT6 Vss AT12 Vss AT20 Vss AT28 Vss AT34 Vss AT38 Vss AV4 Vss AV10 Vss AV18 Vss AV26 Vss AV36